Funktionsrahmen

Dargestellter Umfang:

Ausgew¨ ahlte Bl ¨ocke: ABK, APP, FB, FDEF, FW

System: SG-MED9-1

Projekt: Ea827 TSI

Projektnummer: 5-4420.01/41W038\_PQ35;0

Bearbeiter: Alexander Frick

Abteilung: GS-ES/EAD1

Telefon: 33871

Ausgabedatum: 20.AUG.2004

Translation by Google translate.

Index formatted by Saabman 2019

1072 ADVE 10.20.0 Control of the DV-E with the DLR  
1673 AEKP 27.20.0 Output EKP control  
1789 AES 4.50.0 issue injection  
1879 AEVAB 6.100.9 ssue Injection Ev Blanking  
1904 AEVABU 4.30.0 Output EV shutdown by EGAS monitoring functions  
1905 AEVABZK 1.80.0 Output Ev-Shutdown% MDRED + Complete shutdown by monitoring functions  
1257 ALBK 2.120.1 Control of the charge movement flap  
3246 ALE 7.20.0 outlet detection  
2852 ALSU 2.60.0 Output function LSU  
1683 AMSV 8.70.0 Control of quantity control valve  
284 APP2SV 1.30.0 Provides raw pedal position raw values ​​for OBD testers  
469 ARMD 23.90.0 Moment-based anti-jerk function  
30 ASCETBLK 1.10.0 Description of the ASCET block library  
16 ASCETSDBE 3.15.1 ASCET-SD Description of the ETAS Systemlib blocks  
10 ASCETSDBP 3.13.2 ASCET-SD Description Primitive operators  
1922 ATEV 4.40.0 Control of tank bleed valve (period duration)  
2259 ATM 48.90.2 Exhaust temperature model  
2287 ATMHEX 2.10.2 Modeling the material temperature of the hexagon of the LSU  
2562 ATR 8.80.2 Exhaust gas temperature control  
1800 AWEA 27.20.0 output angle injection control  
2605 BAKH 3.60.1 Operating mode coordination for Catalysts BDE  
2222 BBBO 4.10.2 Operating range Gas detection in oil  
1435 BBDNWS 4.70.1 Readiness Camshaft diagnosis  
3354 BBFEWNE 1.20.0 Processing of Error Messages of the Hardware Driver by KW u. northwest  
300 BBGANG 14.110.1 Operating area aisle  
212 BBHKS 2.20.0 Determining the operational readiness of the BDE mode HKS  
2640 BBHTRIP 1.20.0 Operating condition Heating request Exhaust gas for short test  
113 BBHWONOF 2.30.2 Operating range SG HW Startup and switch off  
286 BBKD 1.50.1 Calculation of the kick-down information  
2597 BBKH 2.50.0 Operating conditions Catalyst heating BDE  
3161 BBKR 17.60.0 Operating conditions Knock control  
2641 BBKW 1.40.0 Operating conditions Catalyst maintained BDE  
914 BBLDR 11.30.0 Operating conditions LDR  
123 BBLOWBAT 2.30.1 Operating range Voltage dip below 5V  
1294 BBSTHDR 1.30.1 Operating conditions High pressure start  
1583 BBSTT 18.10.2 Operating range: Start  
132 BBSYSCON 8.50.1 Operating range System state control  
144 BBSYSREQ 3.30.0 Forwarding conditions for system status  
148 BBWDA 2.10.2 WDA shutdown operating range  
1842 BBZMS 1.40.0 Operating range DMF protection  
201 BDEMAB 2.30.0 BDE mode control: Cancellation of an operating mode  
163 BDEMEN 2.170.0 BDE mode control: Permitted operating modes  
210 BDEMHA 1.60.0 BDE mode control: Heating power requirement  
151 BDEMKO 5.40.0 BDE mode control: Setpoint mode  
204 BDEMST 2.30.0 BDE mode control: Start  
174 BDEMUM 6.10.0 BDE mode control: Coordination of switching  
186 BDEMUS 3.30.0 BDE mode control: Switchover time  
4360 BG41P2SV 1.30.0 Interface for (to) Scan Tool Service Mode $ 01 PID $ 41 monitor status this DCY  
1327 BGARNW 2.70.0 Calculated size Camshaft adaptation requirement  
3686 BGBN 1.10.3 Calculated size of on-board power supply  
192 BGBVG 2.110.0 Calculated sizes Burning limits  
4438 BGCVN 15.10.0 Calculated size Calibration Verification Number CVN  
797 BGDSAD 2.20.2 Calculated Quantities for Pressure Sensor Calibration  
1118 BGDVE 8.50.3 Sizes for DV-E control from learning and test routines  
2996 BGELSV 2.30.1 Calculated size Error LSV  
1901 BGEVAB 4.10.2 Calculation of the Actual Reduction Stage by EV Disconnection  
324 BGFAWU 2.60.1 Calculated size of driver's request  
965 BGFKMS 4.110.2 Calculated size Correction factor mass flow  
4005 BGGNSOL 1.10.0 Calculated size Gearset speed control  
3815 BGKMST 2.30.0 Calculated size: Mileage  
4526 BGKSTDTA 1.70.0 Cold-start detection  
1622 BGKV 14.10.1 Calculated quantity of used fuel  
2329 BGLAMABM 4.30.5 Calculated size lambda in exhaust model  
2940 BGLAMBDA 3.20.1 Calculated size lambda from oxygen signal LSU  
2930 BGLAMOD 1.70.0 Modulation continuous lambda control  
2944 BGLASO 4.90.1 B Lambda nesoll and reciprocal lambda calculation  
1228 BGLBK 2.100.0 Calculated sizes Load movement flap  
616 BGLBZ 11.40.0 Calculated size Battery charge balance  
3805 BGMIL 50.60.0 Calculated sizes; Control MIL (Malfunction Indication Lamp)  
3809 BGMILSF 1.10.1 Calculated quantities; Malfunction Indication Lamp (MIL) Special function  
2224 GMSABG 7.40.3 Calculation of exhaust gas mass flow - bank-dependent  
980 BGMSDK 3.40.2 Calculation mass flow over throttle  
985 BGMSDKS 3.40.4 Calculation of target mass flow via throttle valve  
987 BGMSUGD 3.90.0 Calculation size Mass flow unthrottled  
3312 BGNG 8.30.0 Calculated size Speed ​​gradient  
2626 BGNLLKH 1.60.0 Calculation of the increased LL speed for catalysing (BDE + SRE)  
3292 BGNMOT 8.20.0 Calculated size speed

2244 BGPABG 4.20.1 Calculated size exhaust back pressure  
878 BGPEXT 2.10.0 Calculation of partial pressure by external EGR  
862 BGPIRG 12.20.0 Calculation of internal residual gas content  
918 BGPLGU 1.10.0 Calculation of the basic boost pressure for the supercharged engine  
1002 BGPRGS 3.40.0 Calculation size of internal residual gas setpoint  
781 BGPU 10.50.3 Calculation size Ambient pressure  
803 BGPVD 1.50.1 Pressure output before throttle valve with value range up to 5120 hPa  
3424 BGRBS 5.30.0 Calculated size Wheel acceleration from wheel speed  
1033 BGRFIS 4.10.1 Calculation of relative nominal filling internally  
1044 BGRL2SV 1.30.1 Calculation of Rl reference values ​​for tester output  
881 BGRLFGZS 7.10.0 Calculation of incoming fresh air filling to intake manifold  
894 BGRLG 2.10.0 Calculated size RL-GRADIENT  
1037 BGRLMIN 4.10.1 Calculation of the minimum air rlmin  
1040 BGRLMXS 7.10.0 Calculation of the Maximum Target Filling  
907 BGRLP 21.10.0 Calculation size rlp pre-filled air filling  
993 BGRLSOL 5.100.4 Calculation size target filling  
3277 BGTABST 11.60.0 Calculated size Shutdown time  
1967 BGTEV 8.40.0 Calculation size mass flow TEV  
858 BGTMPK 4.40.0 Fill detection Calculation of temperature compensation  
3617 BGTOCH 1.10.1 Oil temperature in the cylinder head  
3619 BGTOSP 1.10.2 Coordination of the measured value and model value for the oil temperature in oil  
3621 BGTOSPM 1.30.1 Calculation of the oil temperature in the sump (model)  
2311 BGTPABG 5.10.0 Calculated size Dew point in the exhaust system  
3631 BGTUMG 7.100.1 Calculated size Ambient temperature  
491 BGVMAX 1.130.0 Calculation size Maximum speed for VMAX control  
895 BGWDKBA 1.60.2 Calculated Sizes Angle Throttle dam. on Uranschlag  
893 BGWDKHF 4.10.2 C alculation Angle throttle from signal d. Hauptf¨ullungssensors  
901 BGWDKM 1.11.0 Calculation Dk Angle Model  
1316 BGWGWV 1.30.2 Calculated size Angle gas exchange valve  
3287 BGWNE 1.90.1 Calculated basic quantities for angle and speed measurement  
1350 BGWNWVFE 3.20.0 Actual value acquisition camshaft position intake camshaft (s)  
571 BGWPFGR 2.80.3 Calculation values ​​of the recalculated pedal value for FGR  
903 BGWPR 2.30.2 Calculated size Prediction angle  
3315 BISYNC 3.20.2 Speed ​​and Cylinder Counter in 2nd Synchro  
1626 BKS 2.50.1 Demand-driven fuel system  
2561 BTKAT 1.10.2 Operating temperature of the catalysts  
4030 CANECU 1.240.0 CAN send messages and signal definitions  
4087 CANECUR 1.220.0 CAN receive messages  
4208 CANLIB 1.10.0 Library for CAN functions  
4010 CANSEN 1.50.3 Sensor-CAN messages  
4025 CAN\_CONF 1.50.0 CAN channel assignment in the MED9  
1976 COMDTES 2.40.5 Communication DTEV and tank leak diagnosis  
1797 CONCJ 1.60.0 Configuration BDE-HDEV power amplifier  
3993 COWIV 1.80.0 Maintenance Interval Extension  
3759 D2CTR 3.20.0 Diagnostics; Event counter for system observation  
2108 DAAV 1.70.0 Diagnosis AAV valve  
2114 DAAVE 15.10.0 Diagnosis; Plausibility test Check valve Activated charcoal filter Power stage  
2299 DATS 2.40.0 Exhaust gas temperature sensor diagnosis  
1647 DBKS 3.10.4 Diagnosis-demand-controlled fuel system  
1656 DBKSE 3.50.2 Diagnosis Demand-controlled fuel system Power stage  
2422 DCFFLR 1.60.1 Output State Lambda control for Mode $ 01, Mode $ 02, Carb Freeze Frame  
1513 DCV 2.50.0 Crankcase Bleeding Diagnosis  
3296 DDG 19.40.3 Diagnostics of the speed sensor  
1194 DDKV 1.50.1 Diagnosis of throttle contamination  
3714 DDPL 9.30.0 Diagnostics; Plausibility check for permanent care (OBDII)  
1670 DDSBKS 1.10.1 Electrical fault diagnosis of the demand-controlled fuel system  
1738 DDSKV 2.10.2 Diagnosis; High pressure sensor  
1172 DDVE 11.30.0 Diagnosis: EGAS controller DV-E  
3037 DDYLSU 4.100.2 Diagnostics Dynamic behavior of the LSU  
700 DECJ 33.10.0 Diagnosis; Power amplifier CJ4x / 9x  
847 DEGFE 6.110.1 B Diagnosis of input variables Filling detection  
1679 DEKPE 17.10.0 Diagnosis; Electric fuel pump power amplifier  
3760 DFPM 51.30.0 OBDII; Error path Manager  
3774 DFPM2SV 2.10.0 Interface DFPM relevant Information for (to) OBD Service  
3778 DFPMCLA 50.40.0 OBDII Update; class table  
3781 DFPMDAC 50.40.0 Diagnostics Error Path Management; data access  
3783 DFPMEEP 52.10.0 Diagnostics; Error Path Manager, EEPROM storage  
3784 DFPMENV 52.10.0 DFPM Event-noted variables  
3791 DFPMFRZ 50.60.0 Diagnostics Error Path Management; FreezeFrame Logistics  
3791 DFPMOVF 50.20.0 Diagnostics Error Path Management, Memory Overflow  
3792 DFPMTIP 50.40.0 Tester interface package for DFPM50.ff  
3793 DFPMTRG 2.10.0 Trigger table MY2005ff  
1775 DFRST 2.20.4 Diagnostics; Plausibility check Fuel supply system Short test  
1908 DHDEVE 1.80.0 diagnosis; Power amplifier high pressure EV  
2984 DHELSU 100.20.0 Diagnosis of heater input for LSU  
824 DHFM 79.60.1 diagnosis; Plausibility check HFM  
831 DHFMPL 2.110.2 B System diagnostics HFM  
2463 DHKIR 1.50.0 IUMPR for main catalyst diagnosis  
2465 DHKSPSV 2.20.0 MODE6-CAN connection of the main catalytic converter diagnosis  
2765 DHLSHK 7.80.1 Diagnostic Probe heater behind Cat  
2775 DHLSHKE 4.30.3 Diagnostic power amplifier probe heater behind

3705 DHR 5.20.1 Diagnosis; main relay  
2985 DHRLSU 4.100.2 Diagnosis Heating control LSU  
3069 DHRLSUE 4.40.1 Diagnosis heating output stage for systems with BUK power amplifiers  
3053 DICLSU 2.110.0 Dignose: evaluation IC for broadband lambda probe LSU  
4305 DIMCA 50.20.0 Diagnostics; Inspection Maintenance Code, general  
2437 DIMCHLS 3.40.1 Diagnosis; Inspection Maintenance Code, LS Heating Monitoring  
2446 DIMCKAT 4.80.0 Diagnostics; Inspection maintenance code, catalyst monitoring  
2451 DIMCLS 3.30.1 Diagnosis; Inspection maintenance code, lambda sensor monitoring  
1973 DIMCTES 4.90.0 Diagnosis; Inspection Maintenance Code, Tank Discharge System  
3714 DINH 3.30.1 Inhibit Handler  
2815 DKATSP 20.40.0 Catalyst Diagnosis by Mixture Jump  
2836 KATSPEB 10.40.0 Switch-on conditions of the catalyst diagnosis  
680 DKMTR 2.20.1 Diagnosis of coolant temperature control  
3220 DKRA 6.40.1 Diagnosis; Knock control stop  
3224 DKRIC 2.10.1 Diagnostics Knock Sensor Evaluations IC  
3231 DKRS 39.30.2 Diagnosis; Knock sensor (OBDII)  
3244 DKRSPI 1.10.1 Diagnosis Knock control SPI monitoring  
243 DKUPPL 1.40.0 Diagnostic clutch switch  
1768 DKVBDE 3.30.0 Diagnosis fuel supply system BDE  
1780 DKVBDEPL 4.10.2 Diagnostics plausibility check Fuel supply system BDE  
1740 DKVS 29.120.2 Diagnosis; Plausibility check fuel supply systems  
1757 DKVSCOMB 1.30.2 Combination of Fault Path from% DKVS for OBDII Update  
1763 DKVSSC 2.10.4 Release of the cure of GA errors in the context of the similar conditions  
1272 DLBK 4.70.1 Diagnostic charge movement flap  
957 DLDE 9.10.0 Diagnostics LDR power amplifier  
2003 DLDP 20.90.0 OBD II, Tank Discharge Diagnostic Module  
2098 DLDPE 6.20.0 Final stage diagnosis; Overpressure pump of the tank leak diagnosis  
2101 DLDPIR 2.10.0 IUMPR interface for leak diagnosis DLDP  
2104 DLDPSV 1.10.6 MODE6-CAN connection of the OBDII, tank deletion diagnostic module  
948 DLDR 11.30.0 Diagnosis boost pressure control  
959 DLDUV 1.70.0 Diagnosis Diverter valve parallel to the compressor  
962 DLDUVSE 4.10.1 Diagnosis Power stage Diverter valve for compressor  
459 DLLR 37.30.0 Diagnosis: Idle control Detection of blocked controllers  
468 DLLRIR 1.10.0 IUMPR binding of the DLLR  
2778 DLSAHK 18.130.0 Lambda probe aging monitoring behind CAT  
2740 DLSH 33.100.1 Diagnostics; Probe operational readiness behind Cat  
2477 DLSSA 20.50.2 Lambda probe signal output  
2531 DLSSACAN 1.40.1 Signal output (CAN) lambda probes  
3737 DM6CVAL 1.30.1 validation of mode $ 06 - data for CAN  
3738 DM6VAL 5.20.1 Processing diagnostic data for mode $ 06 depending on the validation status  
723 DMBEG 1.10.3 Diagnosis Torque limitation level 1  
3426 DMDDLU 15.10.1 Diagnosis Misfire Detection Difference of the running noise  
3430 DMDFOF 7.40.0 B Diagnosis Misfire Detection Fuel-off Adaptation  
3447 DMDFON 15.40.1 Diagnosis Misfire Detection Fuel-on Adaptation  
3475 DMDLAD 9.10.1 Logic and Delay; Log. Link different blocks for misfire detection  
3478 DMDLFB 8.40.0 Diagnostic Misfire Detection Calculation of uneven running luts and filtered fluts  
3488 DMDLFK 6.30.0 Diagnosis Misfire Detection Correction of the smooth running luts and fluts  
3490 DMDLU 21.60.1 Diagnostic misfire detection; running irregularity  
3502 DMDLUA 18.40.0 Diagnosis Misfire Detection Smoothing Distance Meas  
3506 DMDMIL 20.50.1 B Error handling of misfire detection, activation of MIL and healing  
3600 DMDMON 2.10.0 Diagnostic misfire detection Monitor function  
3565 DMDSTP 31.80.0 Diagnosis Misfire Detection; stop conditions  
3588 DMDSV 1.50.1 Diagnostic misfire detection service  
3596 DMDTSB 14.30.0 Diagnosis Misfire Detection Segment Timing  
3423 DMDUE 18.10.0 Diagnosis Misfire Detection Overview (Overview)  
3601 DMDZAG 5.30.1 Diagnosis misfire detection: Misfire generator  
3809 DMFB 11.30.0 OBDII; MIL alienated  
1729 DMSVE 4.50.0 Diagnostic Power Amplifier MSV  
490 DNMAX 4.30.0 Diagnostics; Plausibility check Maximum speed exceeded  
1498 DNWIR 1.50.0 Diagnosis Camshafts IUMPR connection  
3414 DNWKW 10.20.0 Diagnosis Assignment of camshaft to crankshaft  
1491 DNWSEEIN 4.20.1 Diagnosis of the camshaft output stage (inlet side)  
1453 DNWSEIN 6.120.1 Camshaft control diagnosis (inlet side)  
1448 DNWSZF 4.10.4 Camshaft control diagnosis Error summary  
3335 DPH 24.100.4 B diagnosis; Plausibility check phase sensor  
3001 DPLLSU 2.170.0 Plausibility diagnosis LSU  
792 PLPU 3.40.3 Diagnostics Plausibility check Ambient pressure sensor  
806 DPLPVD 2.30.0 Diagnostics Plausibility check Throttle valve pressure  
3686 DPOWSUP 1.10.2 Diagnostics Encoder supply  
2982 DSALSU 1.40.1 Diagnostic thrust adjustment LSU  
3717 DSCHED 2.110.1 Diagnostic Scheduler  
854 DSELHFS 5.10.0 Selection of the main filling sensor diagnosis  
107 DSGEEP 22.20.0 Diagnostics; Plausibility check SG-EEPROM  
3726 DSM 3.40.0 Diagnostic System Manager  
3811 DSMBDEP 1.40.0 Calculation of BDE Mode Priority  
1603 DSTHDR 1.20.3 High-pressure start diagnostics  
3609 DSWEC 6.20.0 Schlechtwegerk. from Rad-Besch., -> via CAN from ABS SG to Motronic

1990 DTANKL 4.30.3 Diagnosis OBDII error due to empty tank  
2116 DTDW 1.50.0 Fuel Tank Lid Warning  
2171 DTEIR .20.3 IUMPR connection Diagnostics Tank de-aeration valve  
2118 DTEV 3.40.5 Diagnostic Tank Discharge Valve (OBDII)

2168 DTEVE 13.20.0 Diagnosis; Tank bleed valve - output stage

2146 DTEVEB 4.30.1 F Switch-on conditions DTEV

2162 DTEVPAS 1.20.2 Passive diagnosis tank venting valve

3671 DTHM 7.120.0 Diagnosis Thermostat Motor coolant

3824 DTNE 3.10.0 Diagnosis tn - signal output stage

3810 DTOP 1.0.0 Diagnostics; uptime

3828 DUF 6.100.0 Diagnosis from the function monitoring

3030 DULSU 2.80.2 Voltage monitoring continuous lambda probe

3953 DUR 4.30.1 Diagnosis from computer monitoring

3727 DVAL 5.10.0 Diagnostic Validator

68 DVARLC 1.40.2 VW World Custom. MED9.x, Diagnosis variant coding Long coding word

1198 DVE2SV 1.30.0 Interface for OBD II Service Mode $ 01 + $ 02

246 DVFZ 28.140.1 Diagnosis: plausibility check Vehicle speed

3153 DZUEET 2.40.0 Diagnostics D-stop driver

693 DZWPE 3.20.0 Final stage diagnosis; Relay for auxiliary water pump

1544 EAKO 2.30.1 Injection Type Coordinator

2294 EASTKO 1.10.0 Coordination of exhaust temperature sensor error

151 ECUDEV 1.10.0 Recognition of application control units

106 EEPINIKW 1.40.0 EEPROM initialization with characteristic values

4529 EEP\_CONF 5.150.0 EEPROM layout

105 EC 4.0.0 input variables, including their diagnostics

104 EGAG 2.0.0 Input variables in general

964 EGEG 1.0.0 Input variables E-GAS

4245 EGSKO 1.30.1 Coordination between the intervention torques of% GGCEGS,% MDVGSL and% MDASG

3613 EGTE 3.20.0 Input variables Temperature measurement

3332 EPH2LC 1.20.3 Adapter function for DPH (change from "Encoder No." to "Camshaft")

1812 ESAUSG 1.90.2 Output of the injection times and angles to the drivers

1555 ESGRU 23.50.0 Basic injections

1569 ESNSWL 18.10.0 Injection after start and warm-up

1580 ESNSWLA 1.10.2 Optional adapter for re-start / warm-up injection

2937 ESPLANT 1.40.3 Line parameters of the lambda control

1588 ESSTT 37.40.3 Injection time start

1562 ESUK 8.40.1 Injection transition compensation

1552 ESVST 4.30.2 Injection pilot control

1553 ESWE 1.90.1 Injection Thrust shutdown Reinstall

1791 EVABUE 1.20.1 Overview Ev-Shutdown

2174 EVAPDEN 1.30.1 Calculation of the incrementing conditions for the denominator of the EVAP system

1918 EVEKO 2.30.0 Coordination diagnoses HDEV power amplifiers

2291 EXTEMP2SV 1.10.1 Exhaust Gas Temperature Interface for OBD2 Service Mode $ 01

574 FGRABED 1.150.1 Shutdown conditions Vehicle speed controller

567 FGRBESI 1.60.0 Operating signals Travel speed controller

529 FGRFULO 1.130.1 Functional logic of cruise control

548 FGRREGL 1.60.0 Control algorithm Travel speed controller

1966 FITEXFPC 1.10.5 FIT outputs for FPC

2887 FLSUBB 1.100.1 Release of the operational readiness of the LSU

1783 FSSEXFIT 1.20.0 Adapter from Mainfunction FSS to FIT

1050 FUEDK 41.20.1 Filling control (calculation of nominal DK angle)

1059 FUEDKSA 3.40.0 Filling influence via DK, setpoint processing

1061 FUEREG 6.60.4 Filling control

2297 GGATS 7.10.0 Encoder size Exhaust gas temperature sensor

4208 GGCANECU 1.90.1 Encoder sizes CAN transmission information

4222 GGCASR 2.120.1 Transmit CAN signals for ASR / MSR

4247 GGCEGS 5.40.2 Evaluation of the CAN message Transmission

4280 GGCEGSPL 1.90.0 Plausibility check of the CAN message Transmission

4005 GGCGRA 2.20.0 Encoder size GRA control lever with CAN

4290 GGCINS 1.10.0 Evaluation CAN messages from the station wagon

4008 GGCKLA 1.10.0 Evaluation CAN message Climate

4009 GGCLWS 1.10.0 Evaluation CAN message LWS

4291 GGCS 3.50.0 Encoder size Crash sensor

3614 GGCTOL 1.60.0 Granular oil temperature via CAN

3616 GGCTOLAD 1.10.1 Custom interface customization

3630 GGCTUM 4.10.0 Encoder size Ambient temperature via CAN

1727 GGDSKV 2.50.2 Encoder size Fuel pressure sensor

1200 GGDVE 10.50.2 Encoder sizes Throttle valve actuator

238 GGEGAS 9.110.1 Encoder size brake and clutch switch

556 GGFGRH 1.240.0 Encoder sizes Control lever for cruise control

1728 GGFST 11.40.1 Encoder size Tank level

813 GGHFM 76.30.0 Encoder signal HFM

822 GGHFM2SV 1.20.0 Interface% GGHFM to Mode $ 1 / Mode $ 2 Service

3176 GGKR 8.10.0 Encoder sizes Knock control with CC196

1225 GGLBK 6.30.0 Encoder size of the charge movement flap

2671 GGLSH 7.70.0 Encoder size Lambda probe signal (Nernst type) behind Cat

2708 GGLSVFH 1.50.0 Encoder size for SULEV (1ms grid) for probes in front of / behind Cat. behind front cat

2959 GGO2LSU 4.40.1 Encoder size Oxygen signal LSU

265 GGPED 22.20.0 Encoder size Accelerator pedal

778 GGPU 1.50.1 Encoder size function for ambient pressure

800 GGPVD 1.40.0 Encoder size Throttle pressure

2968 GGRTLSU 1.140.1 Encoder size Resistance and temperature of the LSU

3640 GGTFA 18.110.0 Encoder size TFA temperature sensor intake air

3651 GGTFM 46.101.0 Encoder size TFM Temperature sensor Motor (/ coolant)

3685 GGTKA 5.40.0 Encoder size TKA Temperature Cooler output

3693 GGUB 23.10.0 Encoder size Battery voltage, incl. Diagnosis

3698 GGUBR 3.10.1 Encoder sizes and diagnostics On-board voltage via main relay

245 GGVFZG 32.10.2 Encoder size Vehicle speed

1556 GK 21.100.1 Mixture Control

2176 GKEB 4.20.0 Overview Switch-on conditions Mixture control (LR, LRA, TE)

2177 GKRA 5.20.0 Overview Mixture control Control and adaptation

1625 HD .21.0 High pressure control, overview

1713 HDR 9.40.3 High pressure control

1717 HDRPIST 3.30.0 Rail pressure - actual value

1722 HDRPSOL 10.60.0 Fuel pressure setpoint BDE

2659 HLSHK 4.20.2 Probe heater behind Cat

2879 HRLSU 4.150.2 Continuous lambda sensor LSU heating control

1712 HT2KTBKS 1.20.0 Component driver for on-demand fuel supply system

1784 HT2KTCJ830 2.10.0 Interface description CJ830

3151 HT2KTCK110 1.50.0 Component driver CK110 (diagnosable ignition driver)

3816 HT2KTCY315 2.20.1 Component Driver CY315

695 HT2KTDFM 2.10.1 HT2KT for DFM Signal Generator

1211 HT2KTDVE 1.10.0 Interface Hardware driver - component driver DVE

1212 HT2KTDVECJ 1.50.0 Component driver CJ230 Spi bus

810 HT2KTHFM 2.20.0 Interface Hardware Driver - Component Driver HFM

3135 HT2KTIGNI 1.40.0 Component driver Ignition ME (D) 9

4301 HT2KTKMTR 1.40.1 Interface Hardware driver - component driver for KMTR

1221 HT2KTLBK 1.30.0 Interface Hardware Driver - Component Driver LBK

1223 HT2KTLBKCJ 1.10.1 Processing the error flags of the LBK-H bridge (CJ230)

2854 HT2KTLSU 2.20.0 Component drivers CJ120 and CJ125

1697 HT2KTMSV 3.30.0 Hardware driver for component driver Quantity control valve

1506 HT2KTNWS 2.30.3 Interface Hardware driver - Component driver NWS

3317 HT2KTPH 1.161.0 conversion layer hardware driver to component driver camshaft

777 HT2KTPU 1.20.0 Interface Hardware driver Component driver DSU

3823 HT2KTSPIMO 1.10.1 Monitoring SPI masterblocked and node not sent

1925 HT2KTTEV 1.40.2 Interface Hardware driver tank bleed valve

3392 HT2KTTN 1.10.0 Component driver TN signal (speed signal)

3394 HT2KTWNE 5.10.3 Conversion Layer Hardware Driver to Component Driver Crankshaft

3794 IUMPR2TK 1.10.0 IUMPR to Tester Communication interface

3796 IUMPREE 1.30.0 IUMPR - EEPROM storage

3797 IUMPRKF 1.50.0 Core Function IUMPR

619 KMTR 3.430.1 Coolant temperature control

2612 KODOH 1.50.1 B Coordination Double injection Heating for BDE

1874 KOEVAB 2.100.2 Coordination Ev-Shutdown

2629 KOMRH 7.10.0 Coordination of torque reserve for catalyst heating, BDE

92 KONCW 4.230.0 Configuration by Code Words

581 KOS 113.290.0 Air Conditioning Compressor - Control

3212 KRADAP 3.11.0 Knock Control Station Adaptation

3215 KRDY 46.20.0 Knock control Dynamic

3191 KRKE 25.31.0 Knock detection

3203 KRREG 5.10.3 Knock control: Station control

3220 KRZFKT 1.10.0 Special additional functions of knock control

2878 KTGGLSU 1.10.1 ME9 Component Driver for LSU

2663 KTGGLSVFH 2.10.2 KT for encoder sizes GGLSV / GGLSF and GGLSH

2377 KTMHK 2.40.1 Catalyst temperature model Main catalyst

1820 KT\_ES 6.50.0 Component Driver Injection

1624 KVA 52.30.1 Output signal: fuel consumption display

2591 LAKH 10.40.1 Lambda Coordination for Catalysts

2572 LAMBTS 19.130.3 Lambda component protection

2582 LAMKO 21.50.1 Lambda coordination

2588 LAMKOD 1.50.2 Lambda coordination for diagnostic interventions

1542 LAMSDNE 1.10.0 Lambda setpoint after DeNOx end

1535 LAMSOLL 4.10.0 Lambda setpoint

1606 LANSWL 1.40.0 Lambda re-start / warm-up

1537 LASO2SV 1.20.0 Lambda setpoint interface for (to) OBD service

1285 LBKFGS 4.10.0 Release of shift operation by the LBK

1266 LBKSOL 17.10.0 Setpoint specification for the charge movement flap

1220 LBKUE 5.10.0 Overview Cargo movement flap (LBK)

213 LBUESYN 1.20.0 Calculation of runtime bridging signals for all BDE operating modes

942 LDOB 31.40.0 LDR Overboost

919 LDRLMX 8.101.0 Calculation LDR Maximum filling rlmax

931 LDRPID 25.40.1 LDR PID controller

927 LDRPLS 10.40.0 Calculation of nominal boost pressure

940 LDRSTKO 1.10.0 Boost pressure controller coordination

912 LDRUE 34.30.1 LDR overview

941 LDTVMA 27.10.1 Conditioning and Output Duty Cycle

944 LDUVST 7.30.2 F Control of diverter valve

383 LLRBB 505.100.0 Idling control Operating conditions

386 LLRMD 1.43.2 Torque-based no-load control - overview

388 LLRMR 12.220.4 Torque reserve idling control

395 LLRNFA 1.210.0 Speed ​​increase during short trip

425 LLRNSNF 2.10.3 Idle speed tracking

416 LRNSTAT 1.50.0 Idle Station Speed, Coordination and Filtering

400 LLRRM 19.10.2 Idle control Regulator intervention Torque

2557 LOCOS2SV 1.10.2 Interface lambda probes Position for OBD2 Service $ 01 / $ 02

2928 LR2SV 1.20.1 Interface for OBDII service

2195 LRA 140.80.0 B Adaptive pilot control for lambda control

2213 LRA2SV 1.10.2 Interface% LRA for OBD Service

2179 LRAEB 19.30.7 Switch-on conditions Mixture adaptation

2215 LRAPHU 2.60.3 Determination of the physical urgency of mixture adaptation

2689 LRHKEB 3.40.0 Switch-on condition

2901 LRS 21.60.1 Continuous lambda control

2892 LRSEB 20.100.0 Switch-on conditions continuous lambda control

2717 LRSHKC 6.30.0 Lambda control behind Kat steady, version continuous

2732 LRSHKOUT 6.20.2 Encapsulation of the output quantities of the background catalytic converter control

2644 LRSKA 6.90.1 Continuous lambda control Additional function Catalyst extents

1539 LSU2SV 1.10.3 Interface for Scan Tool Mode $ 01 Lambda Actual & Pumping Current

497 MDASG 10.10.1 B Torque automatic transmission ASG

512 MDASGPH 1.100.1

747 MDAUTG 7.80.0 Calculation of the actual torque for the transmission control

729 MDBAS 22.131.0 Calculation of basic quantities for torque interface

515 MDBGRFZG 1.40.0 Vehicle-side torque limitation upwards

521 MDBGRMOT 1.60.0 Motor-specific torque limits

4524 MDBGZL 1.10.1 Torque limit counter

306 MDFAFI 7.10.0 Calculation and change limitation of the driver's desired torque

724 MDFUE 19.80.1 Setpoint specification for air mass from nominal torque

365 MDGEN 2.62.1 Drag torque calculation Generator from KLDF signal

741 MDIST 22.50.1 Engine torque calculation

702 MDKOG 24.180.1 Torque coordination for total interventions

720 MDKOL 26.30.1 Moment coordination at the filling level

775 MDLAM 4.20.0 Torque intervention via lambda

341 MDMAX 2.20.1 Calculation of maximum indexed engine torque

339 MDMIN 10.40.1 Minimum engine torque coordination

342 MDNSTAB 1.41.0 Torque: Speed ​​stabilization

303 MDPED 1.30.0 Accelerator pedal characteristic

760 MDRED 14.120.1 Calculation Reduction stage from torque request

332 MDRWS 1.40.0 Rad desired torque setpoint

482 MDTRAEGM 2.20.0 Dynamic motor torque

528 MDTRIP 1.80.0 Calculation of the torque reserve in the short trip

343 MDVER 20.70.1 Engine loss torque

375 MDVERAD 8.100.1 Adaptation loss torque

354 MDVERB 19.60.0 Required torque of ancillary equipment (eg air conditioning, otherwise consumer)

346 MDWAN 6.200.0 Torque input of the transducer

290 MDZUL 4.120.2 Maximum permissible moment

768 MDZW 7.100.1 Calculation of moment in setpoint angle

746 MRKOMD 1.10.0 Calculation of the scaled desired torque from coordinated moment

1063 MSUDKSOM 1.10.3 Shall mass flow over-critical without torque structure

3372 NLDG 4.30.0 Emergency running speed sensor

216 NLKO 3.120.0 Emergency coordination of the permitted operating modes

3359 NLPH 10.50.7 Emergency Run Phase Encoder

484 NMAXMD 21.60.0 Speed ​​limitation

3294 NMOT2SV 3.20.0 Interface NMOT for OBD Service

432 NSAC 1.10.3 Idling speed AC

436 NSASG 1.10.4 Idling speed ASG automatic gearbox

437 NSBLP 1.10.3 Idle speed cooking protection

438 NSCAT 1.10.2 Idle speed Catalyst heating

439 NSCVT 1.10.3 Idle speed CVT transmission

441 NSGEN 1.10.2 Idle speed generator load

442 NSHTI 2.10.3 Idle speed nominal idle

434 NSKO 1.10.1 Idling speed AC compressor

445 NSLPH 1.10.2 Idling speed Limp-Home

447 NSPTS 1.30.0 Idling speed after-start

449 NSPWG 1.10.3 Idling speed pedal pedal error

450 NSREC 2.20.1 Idle speed with discharged battery

453 NSRNG 1.10.2 Idling nominal speed Maneuvering function

455 NSSTR 2.10.2 Idling nominal speed Short trip

456 NSTST 2.10.1 Idle speed reference tester

1374 NWEVDA 2.10.2 Camshaft restricted adjustment range away Diagnostics Exhaust system

1397 NWEVO 1.180.1 Camshaft: limited adjustment options due to oil pressure

1290 NWFW 6.20.0 Calculation factor angle camshaft

1421 NWSFAT 1.30.2 Camshaft control, setpoint specification by tester

1353 NWSOLLE 11.40.2 Setpoint specification NWS (inlet side)

1286 NWSUE 6.20.0 Overview for camshaft control

1308 NWWUE 8.10.0 Calculation of camshaft overlap

1767 PID41DKV 1.10.2 Definition of the PID41 group for DKVS

1541 PID41HLS 1.10.1 Definition of the PID41 group for the lambda probe heater

2475 PID41KAT 1.20.0 PID $ 41 for catalyst diagnosis

1541 PID41LS 1.10.0 Definition of the PID41 group for Lambda probes

1965 PID41TES 1.10.1 Definition of the PID $ 41 group for the tank detoxification system (EVAP)

3256 RDE 2.30.1 Latch Detection

1838 RKSPLIT 3.10.0 Distribution of relative fuel mass for multiple injection (BDE)

1826 RKTI 32.20.1 Injection duration calculation ti from relative fuel mass rk

2957 RPSLSU 2.30.1 Reference pump current control for the LSU with pumped reference

2974 SALSU 1.130.1 Thrust balance LSU

1214 SREAKT 7.80.2 EGAS: Safety concept, fault reactions

887 SRMHFM 3.10.2 Intake manifold model HFM

889 SRMSEL 3.30.2 Suction tube model selection

3611 SSTDMD 5.30.1 Diagnostic misfire detection: area distributions

1432 SSTNW 1.60.1 Station calculation for camshaft adjustment

1610 STADAP 7.30.0 Start Quantity Adaptation

35 STECK 460.20.0 Pin assignment

34 STEGO 36.20.0 Plug geometry

32 SYABK 8.3.0 Symbols and abbreviations

1793 SYNTIZW 3.20.0 BDE Synchronization Injection / Ignition

109 SYSCON 8.40.0 System state control of the Motronic

82 SYSKON 39.81.3 System constants

3274 SYSYNC 4.40.2 System synchronization

4308 T2ATP 2.10.1 Tester Communication: Access timing parameters

4310 T2DDLI 2.20.0 KWP2000: Dynamically Define Local Identifier

4311 T2DTCS 4.60.0 KWP2000: Read Diagnostic Trouble Codes By Status

4313 T2EDS 3.10.0 Tester Communication: Stop Diagnostic Session

4314 T2EDSA 2.10.1 KWP2000: Stop Diagnostic Session (Application)

4314 T2END 5.10.0 Tester Communication: Stop Communication

4314 T2FCMD 4.40.0 KWP2000: Clear Diagnostic Information

4315 T2ID 4.110.0 KWP2000: Read ECU Information

4319 T2KRLI 2.10.1 Read Data By Local Identifier

4320 T2LID 21.80.0 KWP2000: Read / write Data by Local Identifier

4324 T2REI 1.10.1 Tester Communication: Read ECU Identification

4546 T2RFFD 6.20.0 KWP2000: Read Freze Frame Data

4324 T2RLID 1.20.0 Read Data By Local Identifier

4325 T2RSDTC 3.10.0 Read Status Of DTC

4327 T2RTE 3.10.0 Request Transfer Exit

4327 T2RU 2.30.1 Request Upload

4328 T2SAC 4.50.2 Tester Communication: Security Access

4330 T2SDM 2.80.0 Tester Communication: Set Diagnostic Mode

4331 T2SERV 2.130.0 Service Distributor (Supported Services)

4332 T2SPRL 1.50.1 Stop Routine By Local Identifier

4334 T2STC 1.10.0 Tester Communication: Start Communication

4334 T2STRL 1.150.0 Start Routine By Local Identifier

4345 T2TD 3.20.0 Transfer Data

4345 T2TP 1.10.0 Tester Communication: Tester Present

4346 T2WLID 1.10.1 Write Data By Local Identifier

4346 TC1MOD 31.20.1 tester communication CARB; Fashion 1

4367 TC2MOD 30.30.0 tester communication CARB; Fashion 2

4372 TC3MOD 6.10.2 Tester communication CARB; Mode 3, output error code debounced

4373 TC4MOD 3.30.0 tester communication CARB; Mode 4, erase fault memory

4374 TC5MOD 29.40.0 tester communication CARB; Mode 5, output probe readings

4385 TC6CMOD 1.30.1 tester communication CARB / EOBD; Mode / Service $ 06 via CAN, output check thresholds

4389 TC6MOD 34.50.1 tester communication CARB / EOBD; Mode / Service 6, Issue check thresholds

4414 TC6MODC 1.10.1 Tester communication OBD; Mode / Service $ 06 about CAN, output test results

4418 TC7MOD 11.10.2 Tester communication CARB; Mode 7, issue error code undone

4419 TC8MOD 27.30.0 tester communication CARB; Mode 8, function activations

4423 TC9CON 2.30.0 tester communication CARB; Fashion $ 09 configuration

4425 TC9MOD 15.50.0 tester communication CARB; Mode 9, Request Vehicle Information

4305 TCKOMUE 3.10.0 Tester Communication CARB; Communication setup Overview

4439 TCSORT 6.20.0 tester communication CARB; sort function

1965 TE2SV 1.20.1 Connection to Mode $ 01,02 Tank de-aerating

1935 TEB 110.70.2 Tank de-aerating depending on load

1926 TEBEB 13.50.3 Switch-on conditions Tank de-aerating

2560 TEMPKON 13.20.1 Temperature converter module

3650 TFGG2SV 1.20.0 Interface temperature sensor for (to) OBD service

4440 TKAP 1.40.0 tester communication; Edit customization channels

4443 TKDFA 17.60.0 tester communication; Activate diagnostic function

4451 TKMWL 29.210.2 tester communication; Read measured values

4516 TKSTA 8.70.0 tester communication; Actuator drive

4522 TKSWL 1.60.0 Tester Communication System Values ​​Read

3843 UFACCC 8.10.0 EGAS monitoring concept: ACC Input signal monitoring of the function monitoring

3845 UFEING 12.30.0 B EGAS Monitoring Concept: Input Signal Acquisition for Function Monitoring

3849 UFFGRC 7.20.0 EGAS Monitoring Concept: FGR Monitoring of Function Monitoring

3851 UFFGRE 30.10.0 EGAS monitoring concept: FGR input information for functional monitoring

3864 UFGKC 2.80.0 EGAS Monitoring Concept: Checking Mixture Control in Function Monitoring

3872 UFMIST 12.20.2 EGAS Monitoring Concept: Actual Moment of Function Monitoring

3877 UFMSRC 28.10.2 EGAS Monitoring Concept: MSR intervention monitoring for functional monitoring

3882 UFMVER 4.12.0 EGAS monitoring concept: moment comparison of function monitoring

3885 UFMZF 2.12.0 EGAS monitoring concept: torque filter for function monitoring

3889 UFMZUL 16.30.2 EGAS monitoring concept: permissible moment of functional monitoring

3896 UFNC 4.41.0 EGAS Monitoring Concept: N Monitoring for Function Monitoring

3901 UFNSC 5.40.2 EGAS monitoring concept: post-start monitoring for functional monitoring

3906 UFREAC 11.10.2 EGAS Monitoring Concept: Error Response Monitoring Function

3913 UFRKC 10.20.1 EGAS monitoring concept: target / actual lambda comparison in functional monitoring

3922 UFRKTI 2.30.0 EGAS monitoring concept: Checking fuel mass in functional monitoring

3929 UFRLC 10.10.1 EGAS supervision concept: load signal overv. for functional monitoring

3935 UFSGSC 20.10.3 EGAS Monitoring Concept: SGS Intervention Monitoring for the Function Overview

3941 UFSPSC 19.20.0 EGAS monitoring concept: Pedal setpoint U¨. for functional monitoring

3827 UFUE 17.10.0 EGAS Monitoring Concept: Overview Function Monitoring

3946 UFVARC 5.20.2 EGAS Monitoring Concept: Variant Coding Monitoring of Function Monitoring.

3949 UFZWC 11.10.0 EGAS monitoring concept: ZW monitoring for functional monitoring

3984 UMAUSC 6.40.0 EGAS monitoring concept: shutdown path test monitoring module

3988 UMKOM 11.10.1 EGAS monitoring concept: Question / answer communication between UM and FR

3957 URADCC 17.20.1 EGAS monitoring concept: AD converter test

3962 URCPU 23.10.0 B EGAS surveillance concept: command test with level 2 '

3965 URMEM 4.20.1 EGAS monitoring concept: cyclic storage test

3969 URPAK 2.20.0 EGAS monitoring concept: program flow control

3971 URRAM 4.30.0 EGAS monitoring concept: RAM test

3973 URROM 4.60.0 EGAS monitoring concept: ROM test

3975 URTPU 1.70.0 EGAS monitoring concept: TPU monitoring for functional monitoring

38 VARLC 1.90.1 Variant coding Long coding word (for VW world)

67 VARLCUW 1.10.1 B Variant coding of monitoring-relevant characteristics with a long coding word

264 VFZG2SV 1.20.2 Interface VFZG for OBD Service

495 VMAXMD 5.20.1 Torque request from VMAX control

1068 VPSKO 3.40.1 Coordination of throttling requirements

1690 VSTMSV 3.50.1 feedforward control MSV

1335 WANWKW 21.10.0 Angle adaptation of the camshaft to the crankshaft

1048 WDKSOM 4.20.2 Calculation of throttle setpoint angle without torque structure

4300 WFSCOM 1.20.1 Immobilizer communication

4300 WFSIF 48.40.0 Immobilizer Interface

1375 WNWRE 9.140.0 intake camshaft position control

1843 ZGST 3.10.0 cylinder equalization

1872 ZGSTF9N 1.40.1 Normalization for actual cylinder compensation value from MED9

958 ZLDRD 1.10.0 Cycle counter LDR diagnostics

3073 ZUE 318.20.3 Basic Function - Ignition

3122 ZUESCH 8.10.0 Basic function Ignition in stratified operation

3124 ZUESZ 14.30.0 Zzungung, calculation closing time

3081 ZWBAS 5.70.1 Calculation Zebra Angle for zwbasar

3085 ZWGRU 71.20.0 Basic Angle

3110 ZWHMM 2.20.5 Delta angle as a function of lambda at BDE,

3095 ZWMIN 32.10.0 Calculation of the earliest permitted azimuth angle

3117 ZWOUT 5.70.2 B Calculation of the load angle

3111 ZWSEL 6.30.1 B Calculation ZW after early and late limit

3077 ZWSTT 5.70.1 Ignition in the start

3079 ZWWL 9.20.1 Warm-up Zebra

3076 ZWZYL2SV 1.10.2 Provision of zwzyl1 (ignition angle of cylinder 1) for tester interface