1016 AAGRDC 3.70.0 MED7-Master DC control EGR valve

3378 ABKON 1.10.0 Configuration of the exhaust system

553 ABKVP 1.80.1 Control of brake booster pump

1007 ADAGRLS 4.30.2 Adaptation position sensor EGR valve

377 ADDLGME9Q 1.10.1 Adapter function for diagnostics Running limit HMM operation% DLGHMM for MED9

573 ADVE 8.10.2 Control of the DV-E with the DLR

1618 AEKP 11.20.0 B Output EKP control

1533 AEVAB 6.100.7 Issue Injection Ev Blanking

1555 AEVABU 3.10.0 Output EV shutdown by EGAS monitoring functions

1557 AEVABZK 1.40.0 Output Ev-Shutdown% MDRED + Complete shutdown by monitoring functions

950 AGRPSOL 4.120.0 EGR valve position - setpoint

914 AGRUE 6.20.0 Overview of EGR Packages

1044 ALBK 2.100.2 Control of the charge movement flap

2507 ALE 7.20.0 outlet detection

1918 ALSU 2.10.1 Output function LSU

1600 AMSV 5.100.3 Control quantity control valve

66 ARMD 18.30.0 Moment-based anti-jerk function

3355 ASCETBLK 1.1.0 Description of the ASCET block library

3358 ASCETSDBE 3.12.0 ASCET-SD Description of the ETAS Systemlib block

3372 ASCETSDBP 3.13.0 ASCET-SD Description Primitive operators

1490 ATEV 10.30.3 Control of tank bleed valve (period duration)

1799 ATM 48.50.0 Exhaust temperature model

1825 ATMHEX 2.10.0 Modeling of the material temperature of the hexagon of the LSU

1870 ATR 8.50.2 Exhaust gas temperature control

1509 AWEA 23.20.0 Output Angle injection control

2392 BAKH 3.30.1 Operation mode coordination for Catalysts BDE

956 BBAGR 6.110.2 Switch-on conditions EGR

936 BBAGRMW 2.50.0 Operating Condition EGR Mode Change

1367 BBBO 4.10.1 Operating range Gas detection in oil

867 BBDNWS 1.80.0 Readiness Camshaft diagnosis

3379 BBFEWNE 1.20.0 Processing of Error Messages of the Hardware Driver by KW u. northwest

38 BBGANG 14.100.0 Operating area Gear

375 BBHKS 1.10.0 Determining the operational readiness of the BDE mode HKS

3383 BBHTRIP 1.10.1 Operating condition Heating request Exhaust gas for short test

3384 BBHWONOF 1.60.1 Operating range SG HW Startup and switch off

62 BBKD 1.50.1 Calculation of the kick-down information

2384 BBKH 3.20.2 Operating conditions Catalyst heating BDE

1716 BBKR 9.20.0 Operating conditions Knock control

2400 BBKW 1.40.0 Operating conditions Catalyst maintained BDE

3387 BBLOWBAT 1.30.1 Operating range Voltage dip below 5V

898 BBNWS 4.110.2 Operating conditions for releasing the NWS

3389 BBRCVRY 1.40.1 System Recovery after reset

2217 BBREGNO 1.90.0 Operating range Regeneration NOx catalyst

1090 BBSAWE 46.20.2 Operating range Thrust shutdown / Reinstall

2569 BBSTT 15.10.1 Operating range: Start

3390 BBSYSCON 9.10.0 Operating range System state control

3393 BBWDA 1.40.1 WDA shutdown operating range

119 BBZMS 1.40.0 Operating range DMF protection

367 BDEMAB 2.30.0 BDE mode control: Cancellation of an operating mode

357 BDEMEN 2.150.0 BDE mode control: Permitted operating modes

375 BDEMHA 1.60.0 Heating power-related operating mode requirement

327 BDEMKO 5.30.1 BDE mode control: Setpoint mode

370 BDEMST 2.10.0 BDE operating modes at startup

325 B DEMUE 1.12.0 BDE Mode Selection Overview

339 BDEMUM 2.30.0 BDE mode control: Coordination of switching

351 BDEMUS 3.30.0 BDE mode control: Switchover time

423 BGADAP 5.50.1 Comparison between measured and modeled intake manifold pressure

478 BGAGR 9.90.1 Collection of Cumulations Inclusion of exhaust gas recirculation

969 BGAGRA 4.40.0 Calculation quantity EGR adaptation

983 GAGRDS 1.50.0 Calculation size EGR mass flow from pressure measurement

919 BGAGRSOL 6.150.0 Calculated size EGR nominal rate

984 BGAGRTS 1.10.0 Monitoring the EGR temperature in the (plastic) intake manifold

853 BGARNW 2.70.0 Calculated size Camshaft adaptation requirement

3316 BGBN 1.10.2 Calculated size of on-board power supply

1189 BGBVG 2.110.0 Calculated sizes Burning process limits

3397 BGDSAD 3.10.0 Calculated Quantities for Pressure Sensor Calibration

614 BGDVE 8.10.5 Sizes for DV-E control from learning and test routines

3400 BGELSV 1.40.2 Calculated size Error LSV

1559 BGEVAB 4.10.0 Calculation of the Actual Reduction Stage by EV Disconnection

1139 BGFAWU 2.50.0 Calculated size of driver's request

732 BGFKMS 4.90.0 Calculated size Correction factor mass flow

143 BGGNSOL 1.10.0 Calculated size Gearset speed control

3317 BGKMST 2.30.0 Calculated size: Mileage

1584 BGKV 14.10.0 Calculated quantity of used fuel

2237 BGLAMABM 4.30.4 Calculated size lambda in exhaust model

3406 BGLAMBDA 3.20.2 Calculated size lambda from oxygen signal LSU

3411 BGLAMOD 1.40.2 Modulation continuous lambda control

1154 BGLASO 4.60.1 Calculation lambda nesoll and reciprocal lambda

1053 BGLBK 2.60.0 Calculated sizes Loading motion flap

2814 BGLBZ 8.20.0 Calculated size Battery charge balance

2205 BGMNOREG 1.110.0 Calculation of storage volume NOx from regeneration gas consumption

2226 BGMNOSPM 1.50.0 Calculation of NOx storage content from catalyst model

2233 BGMNOSPS 1.50.0 Stored mass NOx in catalytic converter from NOx signal

1880 BGMSABG 7.40.3 Calculation of exhaust gas mass flow - bank-dependent

727 BGMSDK 3.30.0 Calculation of mass flow over throttle valve

755 BGMSDKS 3.40.4 Calculation of target mass flow via throttle valve

3428 BGMSDSS 1.10.2 Calculation of air mass flow from signal DS-S as skin fill sensor

2467 BGMSNOVK 1.70.0 Calculation size NOx raw mass flow

453 BGMSUGD 3.70.0 Calculation size Mass flow unthrottled

2487 BGNG 8.30.0 Calculated size Speed ​​gradient

289 BGNLLKH 1.50.0 Calculation of the increased LL speed for catalytic combustion (BDE)

2490 BGNMOT 8.20.0 Calculated size speed

488 BGPABG 2.20.0 Calculated size exhaust back pressure

1523 BGPBR 2.10.0 Combustion chamber pressure model BDE

450 BGPEXT 2.10.0 Calculation of partial pressure by external EGR

434 BGPIRG 5.30.0 Calculation of internal residual gas content

2286 BGPNOS 1.60.0 Calculated size Plausibility NOx signal

691 BGPRGS 3.40.0 Calculation size of internal residual gas setpoint

2696 BGRBS 5.30.0 Calculated size Wheel acceleration from wheel speed

939 BGRFIS 2.50.0 Calculation of relative nominal internal filling

746 BGRLFGZS 1.20.2 Calculation of incoming fresh air filling to the intake manifold

519 BGRLG 2.10.0 Calculated size RL-GRADIENT

943 BGRLMIN 1.10.1 Calculation of the minimum air rlmin

946 BGRLMXS 1.50.4 Calculation of the maximum nominal filling

503 BGRLP 21.10.0 Calculation size rlp pre-filled air filling

682 BGRLSOL 5.70.1 Calculation size nominal filling

752 BGRPS 1.40.1 Calculation values ​​for ps controllers

2438 BGSIK 2.200.0 Calculation size sulfur content NOx storage catalytic converter

2822 BGTABST 11.60.0 Calculated size Shutdown time

473 BGTEV 8.40.0 Calculation size Mass flow TEV

459 BGTMPK 7.30.0 Fill detection Calculation of temperature compensation

2750 BGTOL 4.30.0 Calculated size (engine) oil temperature

3429 BGTPABG 1.50.1 Calculated size Dew point in the exhaust system

2773 BGTUMG 7.50.1 Calculated size Ambient temperature

667 BGWDKBA 1.50.0

509 BGWDKHF 4.10.2 Calculation Angle throttle from signal d. Hauptf¨ullungssensors

508 BGWDKM 1.11.0 Calculation Dk Angle Model

861 BGWGWV 1.10.1 Calculated size Angle gas exchange valve

3441 BGWNE 1.90.1 Calculated basic quantities for angle and speed measurement

3445 BGWNWVFE 3.20.0 Actual value acquisition camshaft position intake camshaft (s)

2781 BGWPFGR 2.40.0 Calculation values ​​of the calculated pedal value for FGR

500 BGWPR 2.30.1 Calculated size Prediction angle

2817 BISYNC 3.10.3 Speed ​​and Cylinder Counter in 2nd Synchro

1624 BKS 1.130.0 Demand-controlled fuel system

532 BKV 2.140.1 Pressure control for brake booster

1188 BTKAT 1.10.0 Operating temperature of the catalysts

3503 CANECU 1.90.0 CAN send messages and signal definitions

3536 CANECUR 1.60.1 CAN receive messages

3475 CANSEN 1.50.3 Sensor-CAN messages

1566 CONCJ 3.20.1 Configuration BDE-HDEV power amplifier

3829 COWIV 1.60.1 Maintenance Interval Extension

3318 D2CTR 3.20.0 Diagnostics; Event counter for system observation

3338 DAGRE 16.10.2 Diagnosis; Plausibility check Exhaust return valve - output stage

1003 DAGRKTST 1.30.2 Status byte Short test EGR system

985 DAGRLS 13.50.0 Diagnostic position sensor EGR valve

993 DAGRS 2.110.1 Diagnostic EGR System

3607 DBKS 1.70.0 Diagnostic Demand-Controlled Fuel System

3615 DBKSE 2.10.1 Diagnosis Demand-controlled fuel system output stage

555 DBKVP 2.30.2 Diagnostic brake booster pump

559 DBKVPE 2.10.0 Final stage diagnosis Brake booster pump

3108 DCDACC 2.10.0 Diagnostics; Access to tester data

3275 DCDC 2.10.0 OBDII; Tester code CARB

3417 DCFFLR 1.10.2 Output State Lambda control for Mode $ 01, Mode $ 02, Carb Freeze Frame

3231 DCLA 4.20.0 OBDII; class table

3242 DDCY 15.10.0 OBDII; Fulfillment condition 'driving cycle'

2517 DDG 19.20.2 Diagnostics of the speed sensor

548 DDSBKV 2.30.0 Diagnosis Pressure sensor in the brake booster

1606 DDSKV 1.90.0 Diagnostics; High pressure sensor

511 DDSS 14.90.3 Diagnostics; Pressure sensor in the intake manifold

3321 DDVE 7.30.0 Diagnosis: EGAS controller DV-E

1939 DDYLSU 2.100.2 Diagnostic dynamic behavior of the LSU

3319 DECJ 26.10.0 Diagnosis; Power amplifier CJ4x / 9x

3277 DEPCL 4.10.0 Diagnostics; Electronics Powertrain Control Lamp

3194 DETRE 3.10.0 Diagnostic Power Amplifier Electric Thermostat Control

3234 DFFT 6.30.0 Diagnostics; Freeze frame selection table

3238 DFFTCNV 8.50.0 Diagnostics; Freeze frame table, conversion to bytes

3237 DFFTK 13.30.1 Diagnosis; Custom selection list for freeze frame values

3217 DFPM 15.10.0 OBDII; Error path Manager

3279 DFPMEEP 9.10.0 Diagnostics; Error Path Manager, EEPROM storage

3281 DFPMNL 10.20.0 Diagnostics Error Path Management in the Caster

3280 DFPMOVF 3.20.0 Diagnostics Error Path Management, Memory Overflow

1361 DFRST 2.20.2 Diagnostics; Plausibility check Fuel supply system Short test

3241 DFRZ 20.20.0 OBDII; Description 'freeze frame'

2761 DGGTVHK 2.40.0 Diagnosis of the temperature sensor upstream of the main catalytic converter

1574 DHDEVE 2.20.0 diagnosis; Power amplifier high pressure EV

1968 DHELSU 100.10.1 Diagnosis of heater input for LSU 4.9

2174 DHLSFK 1.30.0 Diagnosis of sensor heating behind front catalytic converter

2181 DHLSFKE 4.20.1 Final stage diagnostics for probe installation location between probe in front of cat and probe h. Kat

2308 DHNOHK 2.90.0 \* Diagnosis heater NOx sensor behind Cat

2792 DHR 4.30.0 Diagnostics; main relay

1927 DHRLSU 3.110.1 Diagnosis Heating control LSU

1936 DHRLSUE 1.80.2 Diagnosis heating output stage for systems with CJ910 / 945 diagnostic ES block, ME9

1952 DICLSU 2.20.0 Dignose: evaluation IC for broadband lambda probe LSU

3244 DIMCA 2.20.0 Diagnostics; Inspection Maintenance Code, general

3250 DIMCAGR 2.30.0 Diagnosis; Inspection Maintenance Code, exhaust gas monitoring system monitoring

3267 DIMCHLS 4.10.0 Diagnostics; Inspection Maintenance Code, LS Heating Monitoring

3252 DIMCKAT 5.10.1 Diagnosis; Inspection maintenance code, catalyst monitoring

3254 DIMCLS 4.10.0 Diagnostics; Inspection maintenance code, lambda sensor monitoring

3247 DIMCTES 4.80.2 Diagnosis; Inspection-Maintenance Code, Tank Discharge System

3215 DINH 2.10.0 Inhibit Handler

2036 DKATFKEB 3.10.0 \* F Switch-on conditions Front catalytic converter diagnosis

2048 DKATSPFK 50.50.0 Diagnosis of the front catalytic converter

1795 DKRA 6.40.1 Diagnosis; Knock control stop

1772 DKRIC 2.10.1 Diagnostics Knock Sensor Evaluations IC

1782 DKRS 39.30.2 diagnosis; Knock sensor (OBDII)

1779 DKRSPI 1.10.1 Diagnosis Knock control SPI monitoring

41 DKUPPL 1.40.0 Diagnostic clutch switch

1607 DKVBDE 3.30.0 Diagnosis fuel supply system BDE

1614 DKVBDEPL 1.50.0 Diagnostic plausibility check Fuel supply system BDE

1346 DKVS 28.50.1 Diagnosis; Plausibility check fuel supply systems

1073 DLBK 4.30.0 Diagnostics Cargo movement flap

378 DLGHMM 1.50.1 Diagnosis Running limit HMM operation

256 DLLR 37.20.0 Diagnostics: Idle control Detected blocked controllers

2140 DLSAFK 1.80.3 Diagnosis: Lambda sensor aging behind front KAT

2071 DLSAHKBD 3.40.0 Lambda probe aging monitoring behind KAT for BDE

2118 DLSF 1.50.1 Diagnosis: Probe readiness behind the front catalytic converter

2188 DLSFV 1.40.1 Diagnosis: detection of the most common lambda probe behind before CAT.

3282 DLSSA 19.40.1 Signal output lambda probes

2001 DLSUV 1.30.1 Detection of exchanged lambda probes before Cat

3343 DLUES1E 2.10.0 Final stage diagnostics Volume control 1

3050 DM6VAL 3.20.2 Processing diagnostic data for mode $ 06 depending on the validation status

324 DMBEG 1.10.2 Diagnosis Torque limitation level 1

2625 DMDDLU 13.40.0 Diagnosis Misfire Detection Difference of the running noise

2654 DMDFOF 5.10.1 Diagnosis Misfire Detection Fuel-off Adaptation

2575 DMDFON 12.30.2 Diagnosis Misfire Detection Fuel-on Adaptation

2652 DMDLAD 8.10.0 Logic and Delay; Log. Link different blocks for misfire detection

2677 DMDLFB 4.40.0 Diagnosis Misfire Detection Calculation of uneven running luts and filtered fluts

2676 DMDLFK 4.30.0 Diagnosis Misfire Detection Correction of the smooth running luts and fluts

2613 DMDLU 17.50.1 Diagnostic misfire detection; runningirregularity

2630 DMDLUA 10.20.0 Diagnosis Misfire Detection Smoothing Distance measurement

2700 DMDMIL 12.50.1 Error handling of misfire detection, activation of MIL and healing

2634 DMDSTP 22.50.0 Diagnosis Misfire Detection; stop conditions

2573 DMDTSB 10.20.1 Diagnosis Misfire Detection Segment Timing

2572 DMDUE 11.20.0 Diagnosis Misfire Detection Overview (Overview)

2686 DMDZAG 3.20.0 Diagnosis misfire detection: Misfire generator

3278 DMFB 11.30.0 OBDII; MIL alienated

3276 DMIL 26.50.0 OBDII; MIL-control

1604 DMSVE 3.10.0 Diagnostic Power Amplifier MSV

239 DNMAX 4.30.0 Diagnostics; Plausibility check Maximum speed exceeded

2289 DNOHK 3.100.1 Diagnosis NOx sensor behind Cat

2478 DNWKW 10.10.0 Diagnosis Assignment of the camshaft to the crankshaft

889 DNWSEEIN 4.10.0 Diagnosis of the camshaft output stage (inlet side)

872 DNWSEIN 4.80.5 Camshaft control diagnosis (inlet side)

895 DNWSZF 1.20.2 Camshaft control diagnosis Error summary

2550 DPH 24.90.1 Diagnosis; Plausibility check phase sensor

1979 DPLLSU 1.90.2 Plausibility diagnosis LSU

1995 DSALSU 1.30.0 Diagnostic thrust balance LSU

3198 DSCHED 2.90.2 Diagnostic Scheduler

528 DSELHFS 2.20.3 Selection of the main filling sensor selection

2324 DSKNO 2.80.0 Diagnostic Memory NOx

3198 DSM 2.10.0 Diagnostic System Manager

3223 DSMBDEP 1.40.0 Calculation of BDE Mode Priority

3340 DSUE 11.20.0 Diagnostics; Intake manifold switching output stage

2694 DSWEC 6.20.0 Schlechtwegerk. from Rad-Besch., -> via CAN from ABS SG to Motronic

1642 DTANKL 4.30.1 Diagnosis OBDII Error due to empty tank

1444 DTEV 39.90.2 Diagnostic Tank Discharge Valve (OBDII)

3334 DTEVE 13.20.0 Diagnosis; Tank bleed valve - output stage

3242 DTIP 1.40.0 OBDII; Tester Interface Package

3822 DTNE 3.10.0 Diagnosis tn - signal output stage

3230 DTOP 1.0.0 Diagnostics; uptime

3233 DTRIG 1.20.0 OBDII; Selectable triggers for error path management

2984 DUF 6.70.1 Diagnosis from function monitoring

1997 DULSU 1.90.0 voltage monitoring continuous lambda probe

3241 DUMWEX 10.10.0 Diagnostic; Extended environmental conditions

2862 DUR 4.20.0 Diagnosis from computer monitoring

3207 DVAL 3.20.0 Diagnostic Validator

561 DVEUE 2.16.0 Overview of the DV-E control

192 DVFZ 17.30.0 Diagnosis: plausibility check vehicle speed

3243 DWUC 14.20.0 OBDII; Fulfillment condition 'warm up cycle'

3770 DZUEET 2.20.1 Diagnosis of the final deceleration driver

3618 EASTKO 1.10.0 Coordination of exhaust temperature sensor error

3396 ECUDEV 1.10.0 Recognition of application control devices

3825 EEPINIKW 1.10.1 EEPROM initialization with characteristic values

3621 EEP\_CONF 5.50.0 EEPROM layout

10 EC 4.0.0 input variables, including their diagnostics

11 EGAG 2.0.0 Input parameters in general

560 EGEG 1.0.0 Input variables E-GAS

409 EGFE 11.40.0 Input variables Filling detection

2725 EGTE 3.20.0 Input variables Temperature measurement

3633 ESAUSG 1.30.1 Output of injection times and angles to the drivers

1098 ESGRU 23.50.0 Basic injections

1120 ESNSWL 1.40.0 B Injection after-start and warm-up

1099 ESSTT 30.20.0 Injection time start

1130 ESUK 8.40.0 Injection transition compensation

1128 ESWE 1.90.1 Injection Thrust shutdown Reinstall

1562 EVABUE 1.20.0 ¨Unsight Ev disconnection

1520 EVEKO 2.20.0 Coordination Diagnostics HDEV power amplifiers

155 FGRABED 1.140.1 Shutdown conditions Travel speed controller

162 FGRBESI 1.50.0 Operating signals Travel speed controller

166 FGRFULO 1.100.1 B Function Logic Vehicle speed controller

185 FGRREGL 1.40.1 Control algorithm Travel speed controller

145 FGRUE 6.20.0 Overview of cruise control

1913 FLSUBB 1.60.1 Release of the operational readiness of the LSU

757 FUEDK 41.20.1 Filling control (calculation of nominal DK angle)

768 FUEDKSA 3.10.2 Filling influence via DK, setpoint processing

766 FUEREG 6.60.2 Filling control

913 GGAGRV 6.60.0 Encoder size EGR valve

3580 GGCANECU 1.60.0 Encoder sizes CAN transmission information

3490 GGCASR 2.30.0 Enclosed CAN signals for ASR / MSR

3592 GGCEGS 1.60.0 Evaluation of the CAN message transmission

3499 GGCGRA 2.20.0 Encoder size GRA control lever with CAN

3596 GGCINS 1.10.0 Evaluation CAN messages from the station wagon

3597 GGCKLA 1.10.0 Evaluation CAN message Climate

3598 GGCLWS 1.10.0 Evaluation CAN message LWS

3599 GGCS 3.30.0 Encoder size Crash sensor

2752 GGCTOL 1.50.1 Granular oil temperature via CAN

2780 GGCTUM 4.10.0 Encoder size Ambient temperature via CAN

1596 GGDSKV 2.40.0 Encoder size Fuel pressure sensor

521 GGDSS 6.160.0 Encoder size Pressure sensor Intake manifold pressure

523 GGDSU 3.40.3 Encoder size Pressure sensor Ambient pressure

563 GGDVE 10.10.3 Encoder sizes Throttle valve actuator

34 GGEGAS 9.70.0 Encoder size brake and clutch switch

147 GGFGRH 1.160.1 Encoder sizes Control lever for cruise control

1641 GGFST 11.40.1 Encoder size Tank level

2754 GGGTS 2.40.0 Encoder size precise temperature signal

3142 GGHLA 1.40.0 Encoder size Heating requirement

1731 GGKR 2.20.2 Encoder sizes Knock control with CC196

1070 GGLBK 6.30.0 Encoder size of the charge movement flap

2012 GGLSF 1.30.3 Encoder size Lambda signal behind front cat

2115 GGLSHNO 1.50.0 Encoder size Lambda signal behind Cat

2027 GGLSVFH 1.30.3 Encoder size for SULEV (1 ms grid) for probes in front of / behind cat. behind front cat

2196 GGNOC 1.170.0 \* Sensor size CAN-NOx sensor behind storage catalytic converter

1899 GGO2LSU 2.20.3 Encoder size Oxygen signal LSU

542 GGPBKV 2.90.1 Encoder size Pressure for brake booster

16 GGPED 10.30.0 Encoder size Accelerator pedal

1907 GGRTLSU 1.90.0 Encoder size Resistance and temperature of the LSU

2743 GGTFA 15.70.0 Encoder size TFA temperature sensor intake air

2746 GGTFAH 1.10.2 Encoder size TFA intake air temperature sensor in the HFM

2726 GGTFM 40.210.0 Encoder size TFM Temperature sensor Motor (/ coolant)

2772 GGTKA 5.30.0 Encoder size TKA Temperature Cooler output

2756 GGTVHK 3.20.0 Encoder size Temperature upstream of the main catalytic converter

2784 GGUB 11.30.1 Sensor size Battery voltage, incl. Diagnosis

2787 GGUBR 1.110.0 Encoder sizes and diagnostics On-board supply voltage via main relay

2782 GGVFZG 27.20.0 Encoder size Vehicle speed

1081 GK 21.60.1 Mixture Control

1199 GKEB 4.20.0 Overview Switch-on conditions Mixture control (LR, LRA, TE)

1586 HD 2.21.0 High pressure control, overview

1587 HDR 2.30.0 High Pressure Control

1594 HDRPIST 2.60.1 Rail pressure - actual value

1589 HDRPSOL 6.20.0 Fuel pressure setpoint BDE

2184 HLSFK 1.40.0 Heater control for probe installation position behind front catalytic converter

1919 HRLSU 4.120.1 Continuous lambda sensor LSU heating control

3644 HT2KTAGR 1.30.0 Interface Hardware Driver - Component Driver AGR

3647 HT2KTBKS 1.10.0 Component driver for on-demand fuel supply system

3647 HT2KTCJ840 1.30.0 Interface Hardware Driver - Component Driver CJ840

3693 T2KTCK110 1.20.1 Component driver CK110 (diagnosable ignition driver)

3730 HT2KTCY315 1.20.0 Component Driver CY315

3680 HT2KTDFM 2.10.1 HT2KT for DFM Signal Generator

3695 HT2KTDVE 1.10.0 Interface Hardware Driver - Component Driver DVE

3654 HT2KTHNOH 1.20.0 Component driver NOx sensor heater behind NOx cat

3712 HT2KTIGNI 1.10.2 Component driver Ignition ME (D) 9

3655 HT2KTKMTR 1.30.1 Interface Hardware Driver - Component Driver for KMTR

3659 HT2KTLBK 1.30.0 Interface Hardware Driver - Component Driver LBK

3661 HT2KTMSV 2.20.2 Hardware driver for component driver Quantity control valve

3686 HT2KTNWS 2.30.3 Interface Hardware driver - component driver NWS

3668 HT2KTPH 1.100.0 B conversion layer hardware driver to camshaft component driver

3711 HT2KTSPIMO 1.10.0 Monitoring SPI masterblocked and node not sent

3685 HT2KTTEV 1.40.2 Interface Hardware driver tank bleed valve

3678 HT2KTTN 1.10.0 Component driver TN signal (speed signal)

3696 HT2KTWNE 1.130.0 Conversion Layer Hardware Driver to Component Driver Crankshaft

3147 KMTR 3.330.2 Coolant temperature control

2403 KODOH 1.31.0 B Coordination Double injection Heating for BDE

1564 KOEVAB 2.20.0 Coordination Ev-Shutdown

2428 KOLASPH 1.20.2 Coordination Lambda Split for Catalytic Fueling (Only for Y-Exhaust System)

2417 KOMRH 5.40.1 Coordination of torque reserve for catalyst heating, BDE

3346 KONCW 4.140.0 Configuration by Code Words

3109 KOS 113.220.0 Air Conditioning Compressor - Control

1768 KRADAP 3.10.0 Knock Control Station Adaption

1764 KRDY 37.11.0 Knock control dynamics

1746 CRC 25.10.2 Knock detection

1757 KRREG 2.20.0 Knock control: Station control

1771 KRZFKT 1.10.0 Special additional functions of knock control

2003 KTGGLSVFH 2.10.2 KT for the encoder sizes GGLSV / GGLSF and GGLSH

1829 KTMHK 2.20.1 Catalyst Temperature Model Main Catalyst

3737 KT\_ES 6.20.0 Component driver injection

3746 KT\_ZUEN 4.10.0 Component driver Ignition Master function for ME9

1585 KVA 52.20.0 Output signal: Fuel consumption display

1171 LAKH 10.40.1 Lambda Coordination for Catalysts

1177 LAMBTS 25.10.1 Lambda component protection

1145 LAMKO 21.30.0 Lambda coordination

1151 LAMKOD 1.40.2 Lambda coordination for diagnostic interventions

1168 LAMSDNE 1.10.0 Lambda setpoint after DeNOx end

1137 LAMSOLL 4.10.0 Lambda setpoint

1165 LANSWL 1.40.0 Lambda re-start / warm-up

1036 LBKFGS 4.10.0 Release of shift operation by the LBK

1037 LBKSOL 13.10.1 Setpoint specification for the charge movement flap

1035 LBKUE 3.30.0 Overview Cargo Movement Flap (LBK)

3227 LBUESYN 1.20.0 Calculation of runtime bridging signals for all BDE operating modes

1198 LGRBY 1.10.0 Travel limit control with ETK bypass

247 LLRBB 505.50.0 Idling control Operating conditions

245 LLRMD 1.43.0 Torque-based idling control - overview

251 LLRMR 12.170.0 Torque reserve idling control

292 LLRNFA 1.210.0 Speed ​​increase during short trip

265 LLRNS 541.260.1 Idling control setpoint speed

296 LLRRM 14.50.0 Idle control Regulator intervention Torque

1322 LRA 134.80.1 Adaptive pilot control for lambda control

1212 LRAEB 18.40.2 Switch-on conditions Mixture adaptation

1339 LRAPHU 1.50.0 Determination of the physical urgency of mixture adaptation

1277 LRFKC 1.20.0 Control behind Cat

1290 LRFKEB 1.50.0 Control behind VorKat

1305 RHKEB 1.80.0 Switch-on condition

1316 LRHKZP 1.10.0 Control behind catalytic converter, variant for desulfating the NOX catalytic converter

1228 LRS 21.30.1 Continuous lambda control

1200 LRSEB 20.60.0 Switch-on conditions continuous lambda control

1253 LRSHKOUT 6.10.1 Routing

1261 LRSKA 8.90.0 Continuous lambda control Additional function Catalyst exhaust

114 MDANF 1.30.0 Approach controller

120 MDASG 3.60.0 Torque automatic transmission ASG

136 MDASGPH 1.90.0

138 MDAUTG 7.80.0 Calculation of the actual torque for the transmission control

93 MDBAS 22.120.1 Calculation of the basic quantities for torque interface

107 MDBGRG 4.150.1 Torque limitation upwards

42 MDFAW 47.10.0 Driver request torque

677 MDFUE 19.80.0 Setpoint specification for air mass from nominal torque

223 MDGEN 2.40.1 Drag torque calculation Generator from KLDF signal

87 MDIST 22.50.1 Engine torque calculation

308 MDKOG 24.100.0 Torque coordination for total interventions

320 MDKOL 26.30.1 Moment coordination at the filling level

105 MDLAM 4.20.0 Torque intervention via lambda

77 MDMAX 2.20.0 Calculation of maximum indexed engine torque

194 MDMIN 10.40.1 Minimum engine torque coordination

196 MDNSTAB 1.51.0 Torque: speed stabilization

1526 MDRED 14.80.0 Calculation Reduction stage from torque request

144 MDTRIP 1.80.0 Calculation of the torque reserve in the short trip

206 MDVER 20.60.0 Engine loss torque

210 MDVERAD 8.60.0 Adaptation loss torque

197 MDVERB 19.10.0 Required torque of auxiliary equipment (eg air conditioning, otherwise consumer)

214 MDWAN 6.110.0 Torque pickup of the transducer

78 MDZUL 4.90.0 Maximum permissible moment

1693 MDZW 7.100.1 Calculation of moment in setpoint angle

2819 MOTOUS 13.20.0 Engine stop

113 MRKOMD 1.10.0 Calculation of the scaled desired torque from coordinated moment

9 MS 3.0.0 Engine Control Overview

12 MSF 11.11.0 Overview Motor Control Functions

772 MSUDKSOM 1.10.3 Shall mass flow over-critical without torque structure

2531 NLDG 4.30.0 Emergency running speed sensor

391 NLKO 3.60.0 \* Emergency coordination of the permitted operating modes

3449 NLPH 10.30.1 Emergency Run Phase Encoder

233 NMAXMD 21.60.0 Speed ​​limitation

831 NWEVO 1.110.2 Camshaft: limited adjustment options due to oil pressure

806 NWFW 1.20.2 Calculation factor angle camshaft

791 NWSFAT 1.30.2 Camshaft control, setpoint specification by tester

808 NWSOLLE 2.140.0 Setpoint specification NWS (inlet side)

802 NWSUE 6.20.0 Overview of camshaft timing

825 NWWUE 5.60.0 Calculation of camshaft overlap

3457 RDE 2.30.1 Rewind detection

1493 RKSPLITS 1.30.0 rk split factor for dual injection

1494 RKTI 20.40.2 Injection duration calculation ti from relative fuel mass rk

1969 RPSLSU 2.20.0 Reference pump current control for the LSU with pumped reference

1971 SALSU 1.130.0 Thrust balance LSU

2334 SKP 2.100.1 Memory validation

2351 SKR 4.60.0 Storage Catalyst Controller

671 SREAKT 7.70.0 EGAS: Safety concept, fault reactions

418 SRMDSS 2.30.0 Intake manifold model DSS

420 SRMHFM 3.10.2 Intake manifold model HFM

414 SRMSEL 3.30.2 Suction tube model selection

411 SRMUE 1.30.0 Intake manifold model overview

1029 SSTAECFS 1.10.0 Landing point calculation for AGR function software

2699 SSTDMD 2.30.0 Diagnosis misfire detection: area distributions

912 SSTNW 1.50.2 Stroke calculation for camshaft adjustment

1108 STADAP 7.30.0 Start Quantity Adaptation

1030 SU 63.80.0 Suction tube switching

3354 SYABK 8.2.0 Symbols and abbreviations

1505 SYNTIZW 3.10.0 BDE Synchronization Injection / Ignition

2806 SYSKON 27.40.1 System constants

2815 SYSYNC 4.40.2 System synchronization

3780 T2ATP 2.10.0 KWP2000: Access timing parameter

3816 T2CBATP 2.10.0 Service AccessTimingParameter for customer boat block

3816 T2CBRD 2.10.0 Request Download (Boot Block)

3818 T2CBREI 2.10.0 Read ECU Identification (Boot Block)

3816 T2CBRRRL 2.10.0 Request Routine Results By Local Identifier (Boot Block)

3819 T2CBRTE 2.10.0 Request Transfer Exit (Boot Block)

3816 T2CBSAC 4.20.0 Security Access (Boot Block)

3818 T2CBSERV 2.10.0 Service Distributor Customer Boot Block (Supported Services)

3818 T2CBSPC 2.10.0 Stop communication for boot block

3815 T2CBSPDS 1.10.0 StopDiagnosticSession for boot block

3815 T2CBSTC 1.10.0 StartCommunication for boot block

3817 T2CBSTDS 2.10.0 StartDiagnosticSession for boot block

3817 T2CBSTRL 2.10.0 Service StartRoutineByLocalIdentifier for customer boat block

3817 T2CBTD 2.10.0 Transfer Data (Boot Block)

3815 T2CBTP 1.10.0 Tester Present for boot block

3778 T2DDLI 2.21.2 KWP2000: Dynamically Define Local Identifier

3782 T2DTCS 4.20.0 KWP2000: Read Diagnostic Trouble Codes By Status

3783 T2EDS 3.10.0 KWP2000: Stop Diagnostic Session

3784 T2EDSA 2.10.0 KWP2000: Stop Diagnostic Session (Application)

3784 T2END 5.10.0 KWP2000: Stop Communication

3785 T2ID 4.60.0 KWP2000: Read ECU Information

3788 T2KRLI 2.10.0 Read Data By Local Identifier

3789 T2LID 21.40.0 KWP2000: Read / write Data by Local Identifier

3793 T2REI 1.10.0 Read ECU Identification (Tester Protocol)

3793 T2RLID 1.20.0 Read Data By Local Identifier

3794 T2RSDTC 1.10.0 Read Status Of DTC

3811 T2RTE 3.10.0 Request Transfer Exit

3814 T2RU 2.20.0 Request Upload

3812 T2SAC 4.40.0 KWP2000: Security Access

3795 T2SDM 2.50.0 Set Diagnostic Mode (Tester Communication)

3796 T2SERV 2.110.0 Service Distributor (Supported Services)

3797 T2SPRL 1.40.0 Stop Routine By Local Identifier

3799 T2STC 1.10.0 Start Communication (Tester Protocol Service)

3799 T2STRL 1.110.0 Start Routine By Local Identifier

3811 T2TD 3.20.0 Transfer Data

3811 T2TP 1.10.0 Tester Present (Tester Protocol)

3792 T2WLID 1.10.1 Write Data By Local Identifier

3001 TC1MOD 20.140.1 tester communication CARB; Fashion 1

3016 TC2MOD 20.71.0 tester communication CARB; Fashion 2

3019 TC3MOD 4.10.0 tester communication CARB; Mode 3, output error code debounced

3020 TC4MOD 3.20.0 tester communication CARB; Mode 4, erase fault memory

3021 TC5MOD 20.40.0 tester communication CARB; Mode 5, output probe readings

3038 TC6MOD 28.30.1 tester communication CARB / EOBD; Mode / Service 6, Issue check thresholds

3043 TC7MOD 9.10.0 Tester Communication CARB; Mode 7, issue error code undone

3043 TC8MOD 23.11.0 tester communication CARB; Mode 8, function activations

3046 TC9MOD 8.30.1 tester communication CARB; Mode 9, Request Vehicle Information

2999 TCKOMUE 2.10.1 Tester communication CARB; Communication setup Overview

2999 TCSORT 3.40.0 tester communication CARB; sort function

1410 TEB 110.10.0 Tank de-aerating depending on load

1402 TEBEB 13.30.0 Switch-on conditions for tank venting

1868 TEMPKON 8.20.1 Temperature converter module

3105 TKAP 1.30.0 tester communication; Edit customization channels

3095 TKDFA 17.50.0 tester communication; Activate diagnostic function

3056 TKMWL 29.120.0 tester communication; Read measured values

3053 TKSTA 8.21.1 tester communication; Actuator drive

3103 TKSWL 1.50.0 Tester Communication System Values ​​Read

2316 TVWNO 1.40.0 Interface adaptation function f. NOx sensor between VW Fct. u. RB Plattf.NOx-Fct.

2869 UFACCC 8.10.0 EGAS monitoring concept: ACC Input signal monitoring of the function monitoring

2866 UFEING 12.30.0 B EGAS Monitoring Concept: Input Signal Acquisition for Function Monitoring

2903 UFFGRC 7.20.0 EGAS Monitoring Concept: FGR Monitoring of Function Monitoring

2889 UFFGRE 30.10.0 EGAS monitoring concept: FGR input information for functional monitoring

2947 UFGKC 2.70.0 Monitoring Mixture correction factors for functional monitoring

2921 UFMIST 12.20.1 EGAS Monitoring Concept: Actual Moment of Function Monitoring

2905 UFMSRC 28.10.2 EGAS Monitoring Concept: MSR intervention monitoring for functional monitoring

2918 UFMVER 4.12.0 EGAS monitoring concept: moment comparison of function monitoring

2926 UFMZF 2.12.0 EGAS monitoring concept: torque filter for function monitoring

2910 UFMZUL 16.20.0 EGAS monitoring concept: permissible moment of functional monitoring

2877 UFNC 4.40.0 EGAS monitoring concept: N monitoring for functional monitoring

2884 UFNSC 5.40.2 EGAS monitoring concept: post-start monitoring for functional monitoring

2955 UFREAC 11.10.0 EGAS Monitoring Concept: Error Response Monitoring Function

2938 UFRKC 10.10.0 Function monitoring: Checking the fuel mass against the LSU signal

2930 UFRKTI 2.30.0 Fuel signal overrun based on ti for functional monitoring

2960 UFRLC 10.10.1 EGAS Monitoring Concept: Load Signal Comp. for functional monitoring

2966 UFSGSC 20.10.1 EGAS Monitoring Concept: SGS Intervention Monitoring for the Function Overview

2871 UFSPSC 19.10.0 EGAS monitoring concept: Pedal setpoint U¨. for functional monitoring

2832 UFUE 17.10.0 EGAS Monitoring Concept: Overview Function Monitoring

2972 UFVARC 3.10.0 EGAS Monitoring Concept: Variant Coding Monitoring of Function Monitoring.

2973 UFZWC 12.10.1 EGAS monitoring concept: ZW monitoring for functional monitoring

2833 UMAUSC 4.10.0 EGAS monitoring concept: shutdown path test monitoring module

2840 UMKOM 4.10.0 EGAS monitoring concept: Question / answer communication between UM and FR

2855 URADCC 17.20.0 EGAS monitoring concept: AD converter test

2861 URCPU 23.11.0 EGAS surveillance concept: command test with level 2 '

2849 URMEM 4.20.1 EGAS monitoring concept: cyclic storage test

2853 URPAK 2.20.0 EGAS monitoring concept: program flow control

2847 URRAM 4.20.0 EGAS monitoring concept: RAM test

2845 URROM 4.30.0 EGAS monitoring concept: ROM test

2977 URTPU 1.60.1 EGAS monitoring concept: TPU monitoring for functional monitoring

3827 VAR 355.20.0 Variant coding

240 VMAXMD 1.30.0 Torque request from VMAX control

722 VPSKO 3.40.0 Coordination of throttling requirements

1597 VSTMSV 2.20.0 feedforward control MSV

2492 WANWKW 19.30.0 Angle adaptation of the camshaft to the crankshaft

771 WDKSOM 4.10.0 Calculation of throttle setpoint angle without torque structure

3819 WFS 48.40.0 Immobilizer

3821 WFSCOM 1.20.1 Immobilizer communication

3821 WFSIF 48.40.0 Immobilizer Interface

777 WNWRE 9.50.1 Inlet camshaft position control

1369 ZGST 3.10.0 Cylinder alignment

1399 ZGSTF9N 2.10.1 Scaling for cylinder compensation actual value from MED9

1656 ZUE 318.20.3 Basic Function - Ignition

1701 ZUESCH 5.40.1 Basic function Ignition in shift operation

3759 ZUESZ 14.20.3 Zzung, calculation closing time

1675 ZWBAS 5.41.1 Calculation Zebra Angle for zwbasar

1661 ZWGRU 56.30.2 basic angle

1660 ZWHMM 2.20.5 Delta angle as a function of lambda at BDE,

1671 ZWLIM 2.32.1 Early ignition angle limit for zwsol at BDE

1704 ZWMIN 14.120.4 Calculation of the latest permitted azimuth angle

1681 ZWOUT 5.50.4 Calculation of the delivery angle

1686 ZWSEL 4.90.3 Calculation ZW after early and late limit

1679 ZWSTT 5.50.0 Attack in the start

1692 ZWWL 9.10.0 warm-up wind angle